# **NodeMcu** #
version 0.9.5
###A lua based firmware for wifi-soc esp8266
Build on [ESP8266 sdk 0.9.5](http://bbs.espressif.com/viewtopic.php?f=5&t=154)<br />
Lua core based on [eLua project](http://www.eluaproject.net/)<br />
File system based on [spiffs](https://github.com/pellepl/spiffs)<br />
Open source development kit for NodeMCU [nodemcu-devkit](https://github.com/nodemcu/nodemcu-devkit)<br />
Flash tool for NodeMCU [nodemcu-flasher](https://github.com/nodemcu/nodemcu-flasher)<br />

wiki: [nodemcu wiki](https://github.com/nodemcu/nodemcu-firmware/wiki)<br />
api: [nodemcu api](https://github.com/nodemcu/nodemcu-firmware/wiki/nodemcu_api_en)<br />
home: [nodemcu.com](http://www.nodemcu.com)<br />
bbs: [Chinese bbs](http://bbs.nodemcu.com)<br />
Tencent QQ group: 309957875<br />

# Summary
- Easy to access wireless router
- Based on Lua 5.1.4 (without *io, math, debug, os* module.)
- Event-Drive programming preferred.
- Build-in file, timer, pwm, i2c, spi, 1-wire, net, mqtt, gpio, wifi, adc, uart and system api.
- GPIO pin re-mapped, use the index to access gpio, i2c, pwm.

# To Do List (pull requests are very welcomed)
- fix wifi smart connect
- add spi module (done)
- add mqtt module (done)
- add coap module
- cross compiler

# Change log
2015-01-27<br />
support floating point LUA.<br />
use macro LUA_NUMBER_INTEGRAL in user_config.h control this feature.<br />
LUA_NUMBER_INTEGRAL to disable floating point support,<br />
// LUA_NUMBER_INTEGRAL to enable floating point support.<br />
fix tmr.time(). #132<br />
fix filesystem length. #113<br />
fix ssl reboots. #134<br />
build pre_build bin.

2015-01-26<br />
applied sdk095_patch1 to sdk 0.9.5.<br />
added LUA examples and modules [by dvv](https://github.com/dvv). <br />
added node.readvdd33() API [by alonewolfx2](https://github.com/alonewolfx2).<br />
build pre_build bin.

2015-01-24<br />
migrate to sdk 0.9.5 release.<br />
tmr.time() now return second(not precise yet). <br />
build pre_build bin.

2015-01-23<br />
merge mqtt branch to master.<br />
build pre_build bin.

2015-01-18<br />
merge mqtt module to [new branch mqtt](https://github.com/nodemcu/nodemcu-firmware/tree/mqtt) from [https://github.com/tuanpmt/esp_mqtt](https://github.com/tuanpmt/esp_mqtt).<br />
merge spi module from iabdalkader:spi. <br />
fix #110,set local port to random in client mode.<br />
modify gpio.read to NOT set pin to input mode automatic.<br />
add PATH env with C:\MinGW\bin;C:\MinGW\msys\1.0\bin;C:\Python27 in eclipse project. resolve #103.

2015-01-08<br />
fix net.socket:send() issue when multi sends are called. <br />
*NOTE*: if data length is bigger than 1460, send next packet AFTER "sent" callback is called.<br />
fix file.read() api, take 0xFF as a regular byte, not EOF.<br />
pre_build/latest/nodemcu_512k_latest.bin is removed. use pre_build/latest/nodemcu_latest.bin instead.

[more change log](https://github.com/nodemcu/nodemcu-firmware/wiki)<br />

##GPIO NEW TABLE ( Build 20141219 and later)

<a id="new_gpio_map"></a>
<table>
  <tr>
    <th scope="col">IO index</th><th scope="col">ESP8266 pin</th><th scope="col">IO index</th><th scope="col">ESP8266 pin</th>
  </tr>
  <tr>
    <td>0 [*]</td><td>GPIO16</td><td>8</td><td>GPIO15</td>
  </tr>
  <tr>
    <td>1</td><td>GPIO5</td><td>9</td><td>GPIO3</td>
   </tr>
   <tr>
    <td>2</td><td>GPIO4</td><td>10</td><td>GPIO1</td>
  </tr>
  <tr>
    <td>3</td><td>GPIO0</td><td>11</td><td>GPIO9</td>
   </tr>
   <tr>
    <td>4</td><td>GPIO2</td><td>12</td><td>GPIO10</td>
  </tr>
  <tr>
    <td>5</td><td>GPIO14</td><td></td><td></td>
   </tr>
   <tr>
    <td>6</td><td>GPIO12</td><td></td><td></td>
  </tr>
  <tr>
    <td>7</td><td>GPIO13</td<td></td><td></td>
   </tr>
</table>
#### [*] D0(GPIO16) can only be used as gpio read/write. no interrupt supported. no pwm/i2c/ow supported.

#Build option
####file ./app/include/user_config.h
```c
// #define FLASH_512K
// #define FLASH_1M
// #define FLASH_2M
// #define FLASH_4M
#define FLASH_AUTOSIZE
...
#define LUA_USE_MODULES
#ifdef LUA_USE_MODULES
#define LUA_USE_MODULES_NODE
#define LUA_USE_MODULES_FILE
#define LUA_USE_MODULES_GPIO
#define LUA_USE_MODULES_WIFI
#define LUA_USE_MODULES_NET
#define LUA_USE_MODULES_PWM
#define LUA_USE_MODULES_I2C
#define LUA_USE_MODULES_TMR
#define LUA_USE_MODULES_ADC
#define LUA_USE_MODULES_UART
#define LUA_USE_MODULES_OW
#define LUA_USE_MODULES_BIT
#endif /* LUA_USE_MODULES */
...
// LUA_NUMBER_INTEGRAL
```

#Flash the firmware
nodemcu_latest.bin: 0x00000<br />
for most esp8266 modules, just pull GPIO0 down and restart.<br />
You can use the [nodemcu-flasher](https://github.com/nodemcu/nodemcu-flasher) to burn the firmware.

Or, if you build your own bin from source code.<br />
0x00000.bin: 0x00000<br />
0x10000.bin: 0x10000<br />

*Better run file.format() after flash*

#Connect the hardware in serial
baudrate:9600

#Start play

####Connect to your ap

```lua
    ip = wifi.sta.getip()
    print(ip)
    --nil
    wifi.setmode(wifi.STATION)
    wifi.sta.config("SSID","password")
    ip = wifi.sta.getip()
    print(ip)
    --192.168.18.110
```

####Manipulate hardware like a arduino
   
```lua
    pin = 1
    gpio.mode(pin,gpio.OUTPUT)
    gpio.write(pin,gpio.HIGH)
    print(gpio.read(pin))
```

####Write network application in nodejs style
   
```lua
    -- A simple http client
    conn=net.createConnection(net.TCP, 0) 
    conn:on("receive", function(conn, payload) print(payload) end )
    conn:connect(80,"115.239.210.27")
    conn:send("GET / HTTP/1.1\r\nHost: www.baidu.com\r\n"
        .."Connection: keep-alive\r\nAccept: */*\r\n\r\n")
```

####Or a simple http server
   
```lua
    -- A simple http server
    srv=net.createServer(net.TCP) 
    srv:listen(80,function(conn) 
      conn:on("receive",function(conn,payload) 
        print(payload) 
        conn:send("<h1> Hello, NodeMcu.</h1>")
      end) 
      conn:on("sent",function(conn) conn:close() end)
    end)
```

####Connect to MQTT Broker

```lua
-- init mqtt client with keepalive timer 120sec
m = mqtt.Client("clientid", 120, "user", "password")

-- setup Last Will and Testament (optional)
-- Broker will publish a message with qos = 0, retain = 0, data = "offline" 
-- to topic "/lwt" if client don't send keepalive packet
m:lwt("/lwt", "offline", 0, 0)

m:on("connect", function(con) print ("connected") end)
m:on("offline", function(con) print ("offline") end)

-- on publish message receive event
m:on("message", function(conn, topic, data) 
  print(topic .. ":" ) 
  if data ~= nil then
    print(data)
  end
end)

-- for secure: m:connect("192.168.11.118", 1880, 1)
m:connect("192.168.11.118", 1880, 0, function(conn) print("connected") end)

-- subscribe topic with qos = 0
m:subscribe("/topic",0, function(conn) print("subscribe success") end)
-- or subscribe multiple topic (topic/0, qos = 0; topic/1, qos = 1; topic2 , qos = 2)
-- m:subscribe({["topic/0"]=0,["topic/1"]=1,topic2=2}, function(conn) print("subscribe success") end)
-- publish a message with data = hello, QoS = 0, retain = 0
m:publish("/topic","hello",0,0, function(conn) print("sent") end)

m:close();
-- you can call m:connect again

```

#### UDP client and server
```lua
-- a udp server
s=net.createServer(net.UDP) 
s:on("receive",function(s,c) print(c) end)
s:listen(5683)

-- a udp client
cu=net.createConnection(net.UDP) 
cu:on("receive",function(cu,c) print(c) end) 
cu:connect(5683,"192.168.18.101") 
cu:send("hello")
```

####Do something shining
```lua
  function led(r,g,b) 
    pwm.setduty(1,r) 
    pwm.setduty(2,g) 
    pwm.setduty(3,b) 
  end
  pwm.setup(1,500,512) 
  pwm.setup(2,500,512) 
  pwm.setup(3,500,512)
  pwm.start(1) 
  pwm.start(2) 
  pwm.start(3)
  led(512,0,0) -- red
  led(0,0,512) -- blue
```

####And blink it
```lua
  lighton=0
  tmr.alarm(1,1000,1,function()
    if lighton==0 then 
      lighton=1 
      led(512,512,512) 
    else 
      lighton=0 
      led(0,0,0) 
    end 
  end)
```

####If you want to run something when system started
```lua
  --init.lua will be excuted
  file.open("init.lua","w")
  file.writeline([[print("Hello, do this at the beginning.")]])
  file.close()
  node.restart()  -- this will restart the module.
```

####With below code, you can telnet to your esp8266 now
```lua
    -- a simple telnet server
    s=net.createServer(net.TCP,180) 
    s:listen(2323,function(c) 
       function s_output(str) 
          if(c~=nil) 
             then c:send(str) 
          end 
       end 
       node.output(s_output, 0)   -- re-direct output to function s_ouput.
       c:on("receive",function(c,l) 
          node.input(l)           -- works like pcall(loadstring(l)) but support multiple separate line
       end) 
       c:on("disconnection",function(c) 
          node.output(nil)        -- un-regist the redirect output function, output goes to serial
       end) 
       print("Welcome to NodeMcu world.")
    end)
```

####Use DS18B20 module extends your esp8266
```lua
    -- read temperature with DS18B20
    t=require("ds18b20")
    t.setup(9)
    addrs=t.addrs()
    -- Total DS18B20 numbers, assume it is 2
    print(table.getn(addrs))
    -- The first DS18B20
    print(t.read(addrs[1],t.C))
    print(t.read(addrs[1],t.F))
    print(t.read(addrs[1],t.K))
    -- The second DS18B20
    print(t.read(addrs[2],t.C))
    print(t.read(addrs[2],t.F))
    print(t.read(addrs[2],t.K))
    -- Just read
    print(t.read())
    -- Just read as centigrade
    print(t.read(nil,t.C))
    -- Don't forget to release it after use
    t = nil
	ds18b20 = nil
    package.loaded["ds18b20"]=nil   
```

####Operate a display via I2c with u8glib
u8glib is a graphics library with support for many different displays.
The integration in nodemcu is developed for SSD1306 based display attached via the I2C port. Further display types and SPI connectivity will be added in the future.

#####I2C connection
Hook up SDA and SCL to any free GPIOs. Eg. [lua_examples/graphics_test.lua](https://github.com/devsaurus/nodemcu-firmware/blob/dev/lua_examples/graphics_test.lua) expects SDA=5 (GPIO14) and SCL=6 (GPIO12). They are used to set up nodemcu's I2C driver before accessing the display:
```lua
sda = 5
scl = 6
i2c.setup(0, sda, scl, i2c.SLOW)
```

#####Library usage
The Lua bindings for this library closely follow u8glib's object oriented C++ API. Based on the u8g class, you create an object for your display type:
```lua
sla = 0x3c
disp = u8g.ssd1306_128x64_i2c(sla)
```
This object provides all of u8glib's methods to control the display.
Again, refer to [lua_examples/graphics_test.lua](https://github.com/devsaurus/nodemcu-firmware/blob/dev/lua_examples/graphics_test.lua) to get an impression how this is achieved with Lua code. Visit the [u8glib homepage](https://code.google.com/p/u8glib/) for technical details.

#####Fonts
u8glib comes with a wide range of fonts for small displays. Since they need to be compiled into the firmware image, you'd need to include them in [app/include/user_config.h](https://github.com/devsaurus/nodemcu-firmware/blob/dev/app/include/user_config.h) and recompile. Simply add the desired fonts to the font table:
```c
#define U8G_FONT_TABLE \
    U8G_FONT_TABLE_ENTRY(font_6x10)  \
    U8G_FONT_TABLE_ENTRY(font_chikita)
```
They'll be available as `u8g.<font_name>` in Lua.
