# DS3231 Module
| Since  | Origin / Contributor  | Maintainer  | Source  |
| :----- | :-------------------- | :---------- | :------ |
| 2015-01-19 | [Tobie Booth](https://github.com/tobiebooth) | [Tobie Booth](https://github.com/tobiebooth) | [ds3231.lua](../../lua_modules/ds3231/ds3231.lua) |

This Lua module provides access to [DS3231](https://datasheets.maximintegrated.com/en/ds/DS3231.pdf) I²C real-time clock.

!!! note
	This module requires `i2c` C module built into firmware.

### Require
```lua
ds3231 = require("ds3231")
```

### Release
```lua
ds3231 = nil
package.loaded["ds3231"] = nil
```

## ds3231.setTime()
Sets the current date and time. If _disableOscillator_ is set to 1 the oscillator will **stop** on battery.

#### Syntax
`ds3231.setTime(second, minute, hour, day, date, month, year[, disableOscillator])`

#### Parameters
- `second`: 00-59
- `minute`: 00-59
- `hour`: 00-23
- `day`: 1-7 (Sunday = 1, Saturday = 7)
- `date`: 01-31
- `month`: 01-12
- `year`: 00-99
- `disableOscillator`: (optional) 0-1, defaults to 0 if omitted

#### Returns
`nil`

#### Example
```lua
i2c.setup(3, 4, scl, i2c.SLOW) -- call i2c.setup() only once

ds3231 = require("ds3231")

-- Set date and time to Sunday, January 18th 2015 6:30PM
ds3231.setTime(0, 30, 18, 1, 18, 1, 15);

-- Don't forget to release it after use
ds3231 = nil
package.loaded["ds3231"] = nil
```

## ds3231.getTime()
Get the current date and time.

#### Syntax
`ds3231.getTime()`

#### Parameters
None

#### Returns
- `second`: integer. Second 00-59
- `minute`: integer. Minute 00-59
- `hour`: integer. Hour 00-23
- `day`: integer. Day 1-7 (Sunday = 1, Saturday = 7)
- `date`: integer. Date 01-31
- `month`: integer. Month 01-12
- `year`: integer. Year 00-99

#### Example
```lua
i2c.setup(3, 4, scl, i2c.SLOW) -- call i2c.setup() only once

ds3231=require("ds3231")

-- Get date and time
second, minute, hour, day, date, month, year = ds3231.getTime();

-- Print date and time
print(string.format("Time & Date: %s:%s:%s %s/%s/%s",
    hour, minute, second, date, month, year))

-- Don't forget to release it after use
ds3231 = nil
package.loaded["ds3231"] = nil
```

## ds3231setAlarm()
Set an alarm to be triggered on SQW pin. _alarm1_ has a precision of **seconds**; _alarm2_ has a precision of **minutes** (`second` parameter will be ignored). Alarms sets gpio.LOW over the SQW pin and let it unchanged until reloaded. When reloaded sets gpio.HIGH. Alarms trigger **only once**, after that, if you want them to trigger again, you need to call `reloadAlarms()` or `setAlarm(...)` again.

Alarm type set the alarm match conditions:

- `ds3231.EVERYSECOND` works only with _alarm1_ and triggers every second;
- `ds3231.EVERYMINUTE` works only with _alarm2_ and triggers every minute (at 00 seconds);
- `ds3231.SECOND` triggers when time match given `seconds` parameter;
- `ds3231.MINUTE` triggers when time match given `seconds` and `minutes` parameters;
- `ds3231.HOUR` triggers when time match given `seconds`, `minutes`, and `hours` parameters;
- `ds3231.DAY` triggers when time match given `seconds`, `minutes`, and `hours` on week day `date/day` parameters;
- `ds3231.DATE` triggers when time match given `seconds`, `minutes`, and `hours` on date (day of the month) `date/day` parameters;

#### Syntax
`ds3231.setAlarm(alarmId, alarmType, seconds, minutes, hours, date/day)`

#### Parameters
- `alarmId`: 1-2
- `alarmType`: 1-7
- `seconds`: 00-59
- `minutes`: 00-59
- `hours`: 00-23
- `date/day`: 01-31 or 1-7 (Sunday = 1, Saturday = 7)

#### Returns
`nil`

#### Example
```lua
i2c.setup(3, 4, scl, i2c.SLOW) -- call i2c.setup() only once

ds3231=require("ds3231")

-- Setting PIN1 to triggers on interrupt when alarm triggers
gpio.mode(1,gpio.INT)
gpio.trig(1,'down',function(level)
  print('Time is passing')
  -- If not reloaded it will be triggered only once
  ds3231.reloadAlarms()
end)

ds3231.setAlarm(2,ds3231.EVERYMINUTE)

-- Don't forget to release it after use
ds3231 = nil
package.loaded["ds3231"] = nil
```

## ds3231.reloadAlarms()
Reload an already triggered alarm. Otherwise it will never be triggered again. There are two different alarms and they have to be reloaded both to let, even only one, to be triggered again. So there isn't a param to select which alarm to reload.

#### Syntax
`ds3231.reloadAlarms()`

#### Parameters
None

#### Returns
`nil`

#### Example
```lua
i2c.setup(3, 4, scl, i2c.SLOW) -- call i2c.setup() only once

ds3231=require("ds3231")

-- Setting PIN1 to triggers on interrupt when alarm triggers
gpio.mode(1,gpio.INT)
gpio.trig(1,'down',function(level)
  print('Time is passing')
  -- If not reloaded it will be triggered only once
  ds3231.reloadAlarms()
end)

ds3231.setAlarm(2,ds3231.EVERYMINUTE)

-- Don't forget to release it after use
ds3231 = nil
package.loaded["ds3231"] = nil
```

## ds3231.enableAlarm()
Enable an already setted alarm with the previous matching conditions. It reloads alarms internally.

#### Syntax
`ds3231.enableAlarm(alarmId)`

#### Parameters
`alarmId`: 1-2

#### Returns
`nil`

#### Example
```lua
i2c.setup(3, 4, scl, i2c.SLOW) -- call i2c.setup() only once

ds3231=require("ds3231")

-- Trigger on x:20:15
ds3231.setAlarm(1,ds3231.MINUTE,15,20)

if badThing == 1 then
  ds3231.disableAlarm(1)
end

if goodThing == 1 then
  ds3231.enableAlarm(1)
end

-- Don't forget to release it after use
ds3231 = nil
package.loaded["ds3231"] = nil
```

## ds3231.disableAlarm()
Disable an already set alarm with the previous matching conditions.

if _alarmId_ is not 1 or 2 it disables both alarms.

**Warning**: `disableAlarm()` prevent alarms to trigger interrupt over SQW pin but alarm itself will triggers at the matching conditions as it could be seen on _status byte_.

#### Syntax
`ds3231.disableAlarm(alarmId)`

#### Parameters
`alarmId: 0-2`

#### Returns
`nil`

#### Example
```lua
i2c.setup(3, 4, scl, i2c.SLOW) -- call i2c.setup() only once

ds3231=require("ds3231")

-- Trigger on x:20:15
ds3231.setAlarm(1,ds3231.MINUTE,15,20)

if badThing == 1 then
  ds3231.disableAlarm(1)
end

if goodThing == 1 then
  ds3231.enableAlarm(1)
end

-- Don't forget to release it after use
ds3231 = nil
package.loaded["ds3231"] = nil
```

## ds3231.getBytes()
Get bytes of control, for debug purpose, and status of DS3231. To see what they means check the [datasheet](http://datasheets.maximintegrated.com/en/ds/DS3231.pdf).

#### Syntax
`ds3231.getBytes()`

#### Parameters
None

#### Returns
- `control`: integer. Control 0-255
- `status`: integer. Status 0-143 (bit 6-5-4 unused)

#### Example
```lua
i2c.setup(3, 4, scl, i2c.SLOW) -- call i2c.setup() only once

ds3231=require("ds3231")

control,status = ds3231.getBytes()
print('Control byte: '..control)
print('Status byte: '..status)

-- Don't forget to release it after use
ds3231 = nil
package.loaded["ds3231"] = nil
```

## da3231.resetStopFlag()
Stop flag on status byte means that the oscillator either is stopped or was stopped for some period and may be used to judge the validity of the timekeeping data. When set to 1 this flag keeps that values until changed to 0. Call `resetStopFlag()` if you need to check validity of time data after that.

#### Syntax
`ds3231.resetStopFlag()`

#### Parameters
None

#### Returns
`nil`

#### Example
```lua
i2c.setup(3, 4, scl, i2c.SLOW) -- call i2c.setup() only once

ds3231=require("ds3231")

control,status = ds3231.getBytes()
if bit.band(bit.rshift(status, 7),1) == 1 then
  print('[WARNING] RTC has stopped')
  ds3231.resetStopFlag()
end

-- Don't forget to release it after use
ds3231 = nil
package.loaded["ds3231"] = nil
```

#### Notes
Other examples of using this module can be found in [ds3231-example.lua](../../lua_modules/ds3231/ds3231-example.lua) and [ds3231-web.lua](../../lua_modules/ds3231/ds3231-web.lua) files.
